# Nmap nmap payload database -*- mode: fundamental; -*-
# $Id: nmap-payloads 38353 2022-02-18 17:38:46Z dmiller $
#
# These payloads are sent with every host discovery or port scan probe
# by default. This database should only include payloads that are
# unlikely to crash services, trip IDS alerts, or change state on the
# server. The idea behind these is to evoke a response using a payload.
# Some of them are taken from nmap-service-probes.
#
# This collection of data is (C) 1996-2022 by Nmap Software LLC.  It
# is distributed under the Nmap Public Source license as provided in
# the LICENSE file of the source distribution or at
# https://nmap.org/npsl/.  Note that this free license does not allow
# incorporation of Nmap or its data files within proprietary
# software. We sell a separate Nmap OEM for that as described
# (including pricing) at https://nmap.org/npsl/.
#
# Each entry begins with a protocol (only "udp" is supported) followed
# by a comma-separated list of ports, followed by one or more quoted
# strings containing the payload. These elements may be broken across
# several lines. For future expansion, additional keywords may follow
# the payload data. Any data following one of these keywords must be on
# the same line as the keyword so that unknown keywords can be ignored
# by the parser. Currently this file contains some entries with the
# "source" keyword to specify a desired source port, but it is not
# honored by Nmap.
#
# Multiple payloads may be defined for a single protocol and port, in
# which case they will be all be sent concurrently. There is a limit
# of 255 payloads per port.
#
# Lines longer than 1024 characters will be ignored.
#
# Example:
# udp 1234 "payloaddatapayloaddata"
#   "payloaddatapayloaddata"
# source 5678

# GenericLines. Use for the echo service.
udp 7 "\x0D\x0A\x0D\x0A"
# DNSStatusRequest
# Sent for TFTP (69) as well due to its ability to provoke an error response
udp 53,69,5353,26198 "\x00\x00\x10\x00\x00\x00\x00\x00\x00\x00\x00\x00"
# DNS VER
udp 53,5353,26198
  "\x77\x77\x01\x00\x00"
  "\x01\x00\x00\x00\x00\x00\x00\x07version\x04bind\x00\x00\x10\x00\x03"

# DHCP INFORM
udp 67
  "\x01\x01\x06\x00"
  "\x01\x23\x45\x67\x00\x00\x00\x00\xff\xff\xff\xff\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x0e\x35\xd4\xd8\x51\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x63\x82\x53\x63\x35\x01"
  "\x08\xff"

# TFTP GET
udp 69 "\x00\x01r7tftp.txt\x00octet\x00"

# QUIC packet with unsupported version Q999
# Also found on 443, but need to check whether DTLS or QUIC is more prevalent
udp 80 "\r12345678Q999\x00"
# RPCCheck
udp 111
  "\x72\xFE\x1D\x13\x00\x00\x00\x00\x00\x00\x00\x02\x00\x01\x86\xA0"
  "\x00\x01\x97\x7C\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00"
# ONCRPC CALL
udp 111,2049,4045,32768-65535
  "\x3e\xec\xe3\xca\x00\x00\x00\x00\x00\x00\x00\x02\x00"
  "\xbc\x61\x4e\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
# NTPRequest
udp 123
  "\xE3\x00\x04\xFA\x00\x01\x00\x00\x00\x01\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\xC5\x4F\x23\x4B\x71\xB1\x52\xF3"
# NTP REQ
udp 123
  "\xd9\x00\x0a\xfa\x00\x00\x00"
  "\x00\x00\x01\x04\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\xc6"
  "\xf1\x5e\xdb\x78\x00\x00\x00"
# DCERPC CALL
udp 135,1025-1199
  "\x05\x00\x0b\x03\x10\x00\x00\x00\x48\x00"
  "\x00\x00\x01\x00\x00\x00\xb8\x10\xb8\x10\x00\x00\x00\x00\x01\x00\x00"
  "\x00\x00\x00\x01\x00\x01\x23\x45\x67\x89\xab\xcd\xef\x01\x23\x45\x67"
  "\x89\xab\xcd\xef\xe7\x03\x00\x00\xfe\xdc\xba\x98\x76\x54\x32\x10\x01"
  "\x23\x45\x67\x89\xab\xcd\xef\xe7\x03\x00\x00"
# NBTStat
udp 137
  "\x80\xF0\x00\x10\x00\x01\x00\x00\x00\x00\x00\x00"
  "\x20CKAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA\x00\x00\x21\x00\x01"
# CIFS NS NAME QUERY UC
udp 137
  "\x01\x91\x00\x00\x00\x01\x00\x00\x00\x00\x00\x00"
  "\x20CKAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA\x00\x00\x21\x00\x01"
# CIFS NS NAME QUERY BC
udp 137
  "\x01\x91\x00\x10\x00\x01\x00\x00\x00\x00\x00\x00"
  "\x20CKAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA\x00\x00\x21\x00\x01"
# SNMPv3GetRequest
udp 161,260,3401
  "\x30\x3A\x02\x01\x03\x30\x0F\x02\x02\x4A\x69\x02\x03\x00\xFF\xE3"
  "\x04\x01\x04\x02\x01\x03\x04\x10\x30\x0E\x04\x00\x02\x01\x00\x02"
  "\x01\x00\x04\x00\x04\x00\x04\x00\x30\x12\x04\x00\x04\x00\xA0\x0C"
  "\x02\x02\x37\xF0\x02\x01\x00\x02\x01\x00\x30\x00"
# SNMP PUBLIC WALK
udp 161,260,3401
  "\x30\x1f\x02\x01\x00\x04\x06public\xa1\x12\x02\x01\x00\x02"
  "\x01\x00\x02\x01\x00\x30\x07\x30\x05\x06\x01\x00\x05\x00"

# Sqlping - disabled because it trips a Snort rule with SID 2049
# ("MS-SQL ping attempt").
# udp 1434 "\x02"

# xdmcp - X Display Manager Control Protocol. Version 1, packet type
# Query (2), no authorization names. We expect a Willing or Unwilling
# packet in reply.
# http://cgit.freedesktop.org/xorg/doc/xorg-docs/plain/hardcopy/XDMCP/xdmcp.PS.gz
udp 177 "\x00\x01\x00\x02\x00\x01\x00"

# Connectionless LDAP - used by Microsoft Active Directory
udp 389
  "\x30\x84\x00\x00\x00\x2d\x02\x01\x07\x63\x84\x00\x00\x00\x24\x04\x00"
  "\x0a\x01\x00\x0a\x01\x00\x02\x01\x00\x02\x01\x64\x01\x01\x00\x87\x0b"
  "objectClass0\x84\x00\x00\x00\x00"


# svrloc
udp 427
  "\x02\x01\x00\x006 \x00\x00\x00\x00\x00\x01\x00\x02en\x00\x00\x00\x15"
  "service:service-agent\x00\x07default\x00\x00\x00\x00"

# DTLS
udp 443,853,3391,4433,4740,5349,5684,5868,6514,6636,8232,10161,10162,12346,12446,12546,12646,12746,12846,12946,13046
  # DTLS 1.0, length 52
  "\x16\xfe\xff\x00\x00\x00\x00\x00\x00\x00\x00\x00\x36"
  # ClientHello, length 40, sequence 0, offset 0
  "\x01\x00\x00\x2a\x00\x00\x00\x00\x00\x00\x00\x2a"
  # DTLS 1.2
  "\xfe\xfd"
  # Random
  "\x00\x00\x00\x00\x7c\x77\x40\x1e\x8a\xc8\x22\xa0\xa0\x18\xff\x93"
  "\x08\xca\xac\x0a\x64\x2f\xc9\x22\x64\xbc\x08\xa8\x16\x89\x19\x3f"
  # Session id length 0, cookie length 0
  "\x00\x00"
  # Cipher suites, mandatory TLS_RSA_WITH_AES_128_CBC_SHA
  "\x00\x02\x00\x2f"
  # Compressors (NULL)
  "\x01\x00"

# Internet Key Exchange version 1, phase 1 Main Mode. We offer every
# combination of (DES, 3DES) and (MD5, SHA) in the hope that one of them will
# be acceptable. Because we use a fixed cookie, we set the association lifetime
# to 1 second to reduce the chance that repeated probes will look like
# retransmissions (and therefore not get a response). This payload comes from
#   ike-scan --lifetime 1 --cookie 0011223344556677 --trans=5,2,1,2 --trans=5,1,1,2 --trans=1,2,1,2 --trans=1,1,1,2
# We expect another phase 1 message in response. This payload works better with
# a source port of 500 or a randomized initiator cookie.
udp 500
  # Initiator cookie 0x0011223344556677, responder cookie 0x0000000000000000.
  "\x00\x11\x22\x33\x44\x55\x66\x77\x00\x00\x00\x00\x00\x00\x00\x00"
  # Version 1, Main Mode, flags 0x00, message ID 0x00000000, length 192.
  "\x01\x10\x02\x00\x00\x00\x00\x00\x00\x00\x00\xC0"
  # Security Association payload, length 164, IPSEC, IDENTITY.
  "\x00\x00\x00\xA4\x00\x00\x00\x01\x00\x00\x00\x01"
  # Proposal 1, length 152, ISAKMP, 4 transforms.
  "\x00\x00\x00\x98\x01\x01\x00\x04"
  # Transform 1, 3DES-CBC, SHA, PSK, group 2.
  "\x03\x00\x00\x24\x01\x01\x00\x00\x80\x01\x00\x05\x80\x02\x00\x02"
  "\x80\x03\x00\x01\x80\x04\x00\x02"
  "\x80\x0B\x00\x01\x00\x0C\x00\x04\x00\x00\x00\x01"
  # Transform 2, 3DES-CBC, MD5, PSK, group 2.
  "\x03\x00\x00\x24\x02\x01\x00\x00\x80\x01\x00\x05\x80\x02\x00\x01"
  "\x80\x03\x00\x01\x80\x04\x00\x02"
  "\x80\x0B\x00\x01\x00\x0C\x00\x04\x00\x00\x00\x01"
  # Transform 3, DES-CBC, SHA, PSK, group 2.
  "\x03\x00\x00\x24\x03\x01\x00\x00\x80\x01\x00\x01\x80\x02\x00\x02"
  "\x80\x03\x00\x01\x80\x04\x00\x02"
  "\x80\x0B\x00\x01\x00\x0C\x00\x04\x00\x00\x00\x01"
  # Transform 4, DES-CBC, MD5, PSK, group 2.
  "\x00\x00\x00\x24\x04\x01\x00\x00\x80\x01\x00\x01\x80\x02\x00\x01"
  "\x80\x03\x00\x01\x80\x04\x00\x02"
  "\x80\x0B\x00\x01\x00\x0C\x00\x04\x00\x00\x00\x01"
source 500
# IPSEC START
udp 500,4500
  "\x31\x27\xfc"
  "\xb0\x38\x10\x9e\x89\x00\x00\x00\x00\x00\x00\x00\x00\x01\x10\x02\x00"
  "\x00\x00\x00\x00\x00\x00\x00\xcc\x0d\x00\x00\x5c\x00\x00\x00\x01\x00"
  "\x00\x00\x01\x00\x00\x00\x50\x01\x01\x00\x02\x03\x00\x00\x24\x01\x01"
  "\x00\x00\x80\x01\x00\x05\x80\x02\x00\x02\x80\x04\x00\x02\x80\x03\x00"
  "\x03\x80\x0b\x00\x01\x00\x0c\x00\x04\x00\x00\x0e\x10\x00\x00\x00\x24"
  "\x02\x01\x00\x00\x80\x01\x00\x05\x80\x02\x00\x01\x80\x04\x00\x02\x80"
  "\x03\x00\x03\x80\x0b\x00\x01\x00\x0c\x00\x04\x00\x00\x0e\x10\x0d\x00"
  "\x00\x18\x1e\x2b\x51\x69\x05\x99\x1c\x7d\x7c\x96\xfc\xbf\xb5\x87\xe4"
  "\x61\x00\x00\x00\x04\x0d\x00\x00\x14\x40\x48\xb7\xd5\x6e\xbc\xe8\x85"
  "\x25\xe7\xde\x7f\x00\xd6\xc2\xd3\x0d\x00\x00\x14\x90\xcb\x80\x91\x3e"
  "\xbb\x69\x6e\x08\x63\x81\xb5\xec\x42\x7b\x1f\x00\x00\x00\x14\x26\x24"
  "\x4d\x38\xed\xdb\x61\xb3\x17\x2a\x36\xe3\xd0\xcf\xb8\x19"
source 500

# Routing Information Protocol version 1. Special-case request for the entire
# routing table (address family 0, address 0.0.0.0, metric 16). RFC 1058,
# section 3.4.1.
udp 520
  "\x01\x01\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x10"

# RMCP ASF ping
udp 623
  "\x06\x00\xff\x06" # RMCP version 6, sequence 0xff, normal RMCP class ASF
  "\x00\x00\x11\xbe" # IAN ASF code 4542
  "\x80\x00\x00\x00" # payload-less ASF presence ping

# IPMI
# RMCP Get Channel Auth Capabilities
udp 623
  "\x06\x00\xff\x07\x00\x00\x00\x00\x00\x00\x00\x00\x00\x09\x20\x18"
  "\xc8\x81\x00\x38\x8e\x04\xb5"

# serialnumberd. This service runs on Mac OS X Server. This probe
# requests the serial number of another server. In response we expect a
# packet starting with "SNRESPS:", followed by some data whose purpose
# is not known.
udp 626 "SNQUERY: 127.0.0.1:AAAAAA:xsvr"

# OpenVPN P_CONTROL_HARD_RESET_CLIENT_V2
# Byte 0; 0x38 opcode
# Byte 1-8: Session ID, random
# Byte 9: Message packet-id array length (0)
# Byte 10-13: Message packet-id (0)
udp 1194 "8d\xc1x\x01\xb8\x9b\xcb\x8f\0\0\0\0\0"
# OpenVPN when in PKI mode and without the "HMAC Firewall" setting enabled
# (tls-auth) should respond to the following probe, which is
# 0x38<8 random bytes><4 null bytes>
udp 1194
  "\x38\x01\x02\x03\x04\x05\x06\x07\x08\x00\x00\x00\x00"

# Citrix MetaFrame application browser service
# Original idea from http://sh0dan.org/oldfiles/hackingcitrix.html
# Payload contents copied from Wireshark capture of Citrix Program
# Neighborhood client application.  The application uses this payload to
# locate Citrix servers on the local network.  Response to this probe is
# a 48 byte UDP payload as shown here:
#
# 0000   30 00 02 31 02 fd a8 e3 02 00 06 44 c0 a8 80 55
# 0010   00 00 00 00 00 00 00 00 00 00 00 00 02 00 06 44
# 0020   c0 a8 80 56 00 00 00 00 00 00 00 00 00 00 00 00
#
# The first 12 bytes appear to be the same in all responses.
#
# Bytes 0x00 appears to be a packet length field
# Bytes 0x0C - 0x0F are the IP address of the server
# Bytes 0x10 - 0x13 may vary, 0x14 - 0x1F do not appear to
# Bytes 0x20 - 0x23 are the IP address of the primary system in a server farm
#                   configuration
# Bytes 0x24 - 0x27 can vary, 0x28 - 0x2F do not appear to
udp 1604
  "\x1e\x00\x01\x30\x02\xfd\xa8\xe3\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"

# RADIUS Access-Request. This is a degenerate packet with no username or
# password; we expect an Access-Reject in response. The Identifier and Request
# Authenticator are both 0. It was generated by running
#   echo 'User-Password = ""' | radclient <ip> auth ""
# and then manually stripping out the password.
#
# Section 2 of the RFC says "A request from a client for which the
# RADIUS server does not have a shared secret MUST be silently
# discarded." So this payload only works when the server is configured
# (or misconfigured) to know the scanning machine as a client.
#
# RFC 2865: "The early deployment of RADIUS was done using UDP port
# number 1645, which conflicts with the "datametrics" service. The
# officially assigned port number for RADIUS is 1812.
udp 1645,1812
  "\x01\x00\x00\x14"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"

# L2TP ICRQ
udp 1701
  "\xc8\x02"
  "\x00\x3c\x00\x00\x00\x00\x00\x00\x00\x00\x80\x08\x00\x00\x00\x00\x00"
  "\x01\x80\x08\x00\x00\x00\x02\x01\x00\x80\x0e\x00\x00\x00\x07"
  "nxp-scan\x80\x0a\x00\x00\x00\x03\x00\x00\x00\x03\x80"
  "\x08\x00\x00\x00\x09\x00\x00"

# UPNP MSEARCH
udp 1900
  "M-SEARCH * HTTP/1.1\r\nHost: 239.255.255.250:1900\r\n"
  "Man: \"ssdp:discover\"\r\nMX: 5\r\nST: ssdp:all\r\n\r\n"

# NFS version 2, RFC 1831. XID 0x00000000, program 100003 (NFS), procedure
# NFSPROC_NULL (does nothing, see section 2.2.1), null authentication (see
# section 9.1).
udp 2049
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x02\x00\x01\x86\xA3"
  "\x00\x00\x00\x02\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
  "\x00\x00\x00\x00\x00\x00\x00\x00"

# GPRS Tunneling Protocol (GTP)
udp 2123,2152
# GTPv1, protocol 1
"\x32"
# EchoRequest
"\x01"
# message length
"\x00\x04"
# Tunnel endpoint identifier
"\x00\x00\x42\x00"
# sequence number
"\x13\x37"
# N-PDU number
"\x00"
# next extension header type
"\x00"

# GPRS Tunneling Protocol (GTP) "prime" v2
# This same packet can be used for GTP v2 on ports 2123 and 2152 if you change
# the first byte from \x4e to \x40
udp 3386
# GTP'v2
"\x4e"
# EchoRequest
"\x01"
# message length
"\x00\x04"
# sequence number
"\xde\xfe\xc8\x00"

# Freelancer game server status query
# http://sourceforge.net/projects/gameq/
# (relevant files: games.ini, packets.ini, freelancer.php)
udp 2302 "\x00\x02\xf1\x26\x01\x26\xf0\x90\xa6\xf0\x26\x57\x4e\xac\xa0\xec\xf8\x68\xe4\x8d\x21"

# Apple Remote Desktop (ARD)
udp 3283 "\0\x14\0\x01\x03"

# STUN Binding request, see RFC 5389 Section 6
# message type = 0x001, Binding (see Section 18.1)
# message length = 0
# magic cookie = 0x2112a442
# transaction ID = "\x00"*12
udp 3478 "\x00\x01\x00\x00\x21\x12\xa4\x42\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"

# Sun Service Tag Discovery protocol (stdiscover)
# http://arc.opensolaris.org/caselog/PSARC/2006/638/stdiscover_protocolv2.pdf
# Would work better with a varying cookie; the second and later sends of this
# probe will be interpreted as resends by the server and will be ignored.
udp 6481 "[PROBE] 0000"

# NAT-PMP external IP address request. See section 3.2 of
# http://files.dns-sd.org/draft-cheshire-nat-pmp.txt.
udp 5351 "\x00\x00"

# DNS Service Discovery (DNS-SD) service query, as used in Zeroconf.
# Transaction ID 0x0000, flags 0x0000, 1 question: PTR query for
# _services._dns-sd._udp.local. If the remote host supports DNS-SD it will send
# back a list of all its services. This is the same as a packet capture of
#   dns-sd -B _services._dns-sd._udp .
# See section 9 of
# http://files.dns-sd.org/draft-cheshire-dnsext-dns-sd.txt.
# This first probe is a QU probe, meaning a unicast response is desired
udp 5353
  "\x00\x00\x00\x00\x00\x01\x00\x00\x00\x00\x00\x00"
  "\x09_services\x07_dns-sd\x04_udp\x05local\x00\x00\x0C\x80\x01"
# This second probe is a QM probe, meaning a unicast response is desired
udp 5353
  "\x00\x00\x00\x00\x00\x01\x00\x00\x00\x00\x00\x00"
  "\x09_services\x07_dns-sd\x04_udp\x05local\x00\x00\x0C\x00\x01"

# PCANY STATUS
udp 5632 "ST"

# CoAP GET .well-known/core
udp 5683 "@\x01\x01\xce\xbb.well-known\x04core"

# UT2K PING
udp 7777 "None\x00"

# Ubiquiti Discovery Service - v1
udp 10001 "\x01\x00\x00\x00"

# Amanda backup service noop request. I think that this does nothing on the
# server but only asks it to send back its feature list. In reply we expect an
# ACK or (more likely) an ERROR. I couldn't find good online documentation of
# the Amanda network protocol. There is parsing code in the Amanda source at
# common-src/security-util.c. This is based on a packet capture of
#   amcheck <config> <host>
udp 10080
  "Amanda 2.6 REQ HANDLE 000-00000000 SEQ 0\n"
  "SERVICE noop\n"

# VxWorks Wind River Debugger
udp 17185
# Random XID
"\x00\x00\x00\x00"
# RPC version 2 procedure call
"\x00\x00\x00\x00\x00\x00\x00\x02"
# WDB version 1
"\x55\x55\x55\x55\x00\x00\x00\x01"
# WDB_TARGET_PING
"\x00\x00\x00\x00"
# RPC Auth NULL
"\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"
# Checksum
"\xff\xff\x55\x13"
# WDB wrapper (length and sequence number)
"\x00\x00\x00\x30\x00\x00\x00\x01"
# Empty data?
"\x00\x00\x00\x02\x00\x00\x00\x00\x00\x00\x00\x00"
# VXWORKS DEBUG (alternative?)
udp 17185
  "\x72\x37\x72\x37\x00\x00\x00"
  "\x00\x00\x00\x00\x02\x55\x55\x55\x55\x00\x00\x00\x01\x00\x00\x00\x01"
  "\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\xff"
  "\xff\x55\x10\x00\x00\x00\x3c\x00\x00\x00\x03\x00\x00\x00\x02\x00\x00"
  "\x00\x00\x00\x00\x00\x00"

# Quake 2 and Quake 3 game servers (and servers of derived games like Nexuiz).
# Gets game information from the server (see probe responses in
# nmap-service-probes). These services typically run on a base port or a
# few numbers higher.
# Quake 2. Typical ports: 27910-27914.
udp 27910-27914 "\xff\xff\xff\xffstatus"
# Quake 3. Typical ports:
# 26000-26004: Nexuiz
# 27960-27964: Various games
# 30720-30724: Tremulous
# 44400: Warsow
udp 26000-26004,27960-27964,30720-30724,44400 "\xff\xff\xff\xffgetstatus"

# Murmur 1.2.X (Mumble server)
# UDP ping. "abcdefgh" is an identifier. See
# http://mumble.sourceforge.net/Protocol.
udp 64738 "\x00\x00\x00\x00abcdefgh"

# Ventrilo 2.1.2+
# UDP general status request (encrypted).
# See http://aluigi.altervista.org/papers.htm#ventrilo
udp 3784
"\x01\xe7\xe5\x75\x31\xa3\x17\x0b\x21\xcf\xbf\x2b\x99\x4e\xdd\x19\xac\xde\x08\x5f\x8b\x24\x0a\x11\x19\xb6\x73\x6f\xad\x28\x13\xd2\x0a\xb9\x12\x75"

# Kademlia (kad) as used by various P2P applications.  Send a Kademlia ping
# 4665, 4666, 4672, 6429: eDonkey/eMule and variants
udp 4665,4666,4672,6429 "\xE4\x60"

# TeamSpeak 2
# UDP login request
# See http://wiki.wireshark.org/TeamSpeak2
udp 8767
"\xf4\xbe\x03\x00\x00\x00\x00\x00\x00\x00\x00\x00\x01\x00\x00\x002x\xba\x85\tTeamSpeak\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\nWindows XP\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x02\x00\x00\x00 \x00<\x00\x00\x01\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x08nickname\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00"

# TS3INIT1
udp 9987
"TS3INIT1\x00\x65\x00\x00\x88\x0a\x39\x7b\x0f\x00\x5b\x55\x72\xef\xdc\x78\x32\x6b\x00\x00\x00\x00\x00\x00\x00\x00"

# TeamSpeak 3
# UDP login request (encrypted)
# http://seclists.org/nmap-dev/2013/q3/72
udp 9987
"\x05\xca\x7f\x16\x9c\x11\xf9\x89\x00\x00\x00\x00\x02\x9d\x74\x8b\x45\xaa\x7b\xef\xb9\x9e\xfe\xad\x08\x19\xba\xcf\x41\xe0\x16\xa2\x32\x6c\xf3\xcf\xf4\x8e\x3c\x44\x83\xc8\x8d\x51\x45\x6f\x90\x95\x23\x3e\x00\x97\x2b\x1c\x71\xb2\x4e\xc0\x61\xf1\xd7\x6f\xc5\x7e\xf6\x48\x52\xbf\x82\x6a\xa2\x3b\x65\xaa\x18\x7a\x17\x38\xc3\x81\x27\xc3\x47\xfc\xa7\x35\xba\xfc\x0f\x9d\x9d\x72\x24\x9d\xfc\x02\x17\x6d\x6b\xb1\x2d\x72\xc6\xe3\x17\x1c\x95\xd9\x69\x99\x57\xce\xdd\xdf\x05\xdc\x03\x94\x56\x04\x3a\x14\xe5\xad\x9a\x2b\x14\x30\x3a\x23\xa3\x25\xad\xe8\xe6\x39\x8a\x85\x2a\xc6\xdf\xe5\x5d\x2d\xa0\x2f\x5d\x9c\xd7\x2b\x24\xfb\xb0\x9c\xc2\xba\x89\xb4\x1b\x17\xa2\xb6"

# Memcached
# version request (shorter response than stats)
# https://github.com/memcached/memcached/blob/master/doc/protocol.txt
udp 11211
"\0\x01\0\0\0\x01\0\0version\r\n"

# Steam, typically using a port in 27015-27030.  Send a "Source Engine query"
udp 27015-27030
  "\xff\xff\xff\xffTSource Engine Query\x00"

# TRIN00 UNIX PING
udp 27444 "png l44adsl"

# BO PING
udp 31337
  "\xce\x63\xd1\xd2\x16\xe7\x13\xcf\x38"
  "\xa5\xa5\x86\xb2\x75\x4b\x99\xaa\x32\x58"

# TRIN00 WIN PING
udp 34555 "png []..Ks"

# Beckhoff ADS discovery request
# https://github.com/ONE75/adsclient/blob/master/src/AdsClient.Finder/DeviceFinder.cs#L49-L64
udp 48899
"\x03\x66\x14\x71\x00\x00\x00\x00\x01\x00\x00\x00\x00\x00\x00\x00\x01\x01\x10\x27\x00\x00\x00\x00"
